TRIPLE GHOST

A. Hardware :

# 1. TP-Link TL-MR3040 / TP-Link TL-MR11U

Specs

Atheros AR7240 @ 400 MHz

32 MiB RAM

4 MiB Flash

100MBit Ethernet

USB 2.0

SoC: Atheros AR9331 rev1

802.11 b/g/n 150Mbps

Powered via mini-USB (5V) or Li-ion Battery included (4-5 hours)

uses included >=  Sandisk 4GiB USB storage device

2. TP-Link TL-722N V1

Antena Gain 4 dB

Freq 2.400-2.4835GHz

Signyal rate 11n: Up to 150Mbps, 11g: Up to 54Mbps., 11b: Up to 11Mbps.

Transmit Power <20dBm

USB 2.0

Chipset Atheros AR9271 (Support Mode Monitor and Injection)

Antenna Type Detachable Omni Directional (RP-SMA)

B. Software/Firmware:

1. OpenWRT 12.09 "Attitude Adjustment," dirilis pada tanggal 25 April 2013

2. MiniPwner Build Scripts oleh Kevin Bong

3. Antarmuka web nanas Wifi oleh Hak5

4. Sword oleh zer0byte

c. Package Include

Nmap network scanner

Tcpdump sniffer

Netcat Hacker’s swiss army knife

aircrack Wireless network analysis

kismet Wireless network analysis

openvpn VPN Client and Server

dsniff suite of sniffing and spoofing tools, including arpspoof

nbtscan NetBIOS Network Scanner

snort Sniffer, Packet Logger, Intrusion Detection System

karma Wireless Sniffing Tool

samba2-client Windows File Sharing Client

elinks Text Based Web Browser

openssh-sftp-client Secure File Transfer Client

etc.

**HOW TO**

A. Membangun Ulang (Jika triple Ghost Error)

1. login via telnet atau ssh dan lakukan a firstboot && reboot

2. Re-flash Triple Ghost dengan [attitude-adjustment](http://downloads.openwrt.org/attitude_adjustment/12.09/ar71xx/generic/).

3. Download firmware dan nyalakan untuk diunduh di mesin lokal Anda dengan netcat: nc -l < filename.bin 6666

4. Dari router Anda, pindahkan firmware dari mesin Anda dengan netcat:  
cd /tmp

nc 192.168.1.111 6666 > filename.bin

mtd -r write filename.bin firmware

5. Download image dd ini dan tuliskan ke Sandisk Cruzer Fit 8GB (gunakan Linux)